**Addendum: No. 01**

|  |  |  |  |
| --- | --- | --- | --- |
| **No** | **Clause** | **Existing Clause** | **Amended Clause** |
| 1 | 1.1 | Delete the following sentence of the 4th paragraph.  *“A drawing is enclosed with the bidding document. However, prior to fabricate, the dimensions shall be validated by the successful bidder with the available sample.”* | Insert following paragraph as the 4th para of the section 1.1  *“A drawing is enclosed with the bidding document. However, prior to fabricate, the dimensions shall be validated by the successful bidder with the available sample and visiting the Trincomalee Site”* |
| 2 | 1.2 | Delete the following section;  *“In order to seal the storage tanks, 04 manhole covers shall be used per tank with gaskets. Contractor shall Supply 20 Numbers of Elliptical Manhole covers and, each manhole cover shall be comprised with 02 Yokes, 02 Nuts and 02 Bolts & 01 Nos. Gasket (Material: Klingersil K-1000 gasket 2.5mm thickness).*   * *If the manholes are casted, the quality management program shall be provided*   *&*   * *If the Manholes covers are fabricated by carbon steel, Design calculation shall be provided.* * *However, either in both casting or carbon steel fabrication, the design shall be certified by a Charted Mechanical Engineer.*   *Initially, only Four (4) manhole cover units shall be supplied. Once the hydraulic testing for a one particular tank is completed using the supplied covers, the balance sixteen (16) units shall be fabricated & supplied.”* | Insert following section as the section 1.2  *“In order to seal the storage tanks, 04 manhole covers shall be used per tank with gaskets. Contractor shall Supply 20 Numbers of Elliptical Manhole covers (25mm thickness) and, each manhole cover shall be comprised with 02 Yokes, 02 Nuts and 02 Bolts & 01 Nos. Gasket (Material: Klingersil K-1000 gasket 2.5mm thickness).*  *Prior to fabricate Manholes covers, a Design calculation certified by a Chartered Mechanical Engineer shall be submitted for the approval of CPC.*  ***Fabrication Materials:***   * *Manhole Cover/Yokes: ASTM A283 Grade C or equivalent* * *Bolt: ASTM A193 B7 or equivalent* * *Nut: ASTM A194 2H Heavy Hex Nut or equivalent* * *Gasket: Klingersil K-1000 gasket 2.5mm thickness or equivalent*   *Initially, only Four (4) manhole cover units shall be supplied. Once the hydraulic testing for one particular tank is completed using the supplied covers, the balance sixteen (16) units shall be fabricated & supplied.”* |
| 3 | 2.2 | Delete the following sentence in 2.2  *“05% of the Payment shall be made upon submission of Quality Management Program or Design Calculation certified by a Chartered Mechanical Engineer”* | Insert the following para as the second para of 2.2  *“05% of the Payment shall be made upon submission of Design Calculation certified by a Chartered Mechanical Engineer”* |